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SRI LANKA STATE TRADING (General) CORPORATION LTD
INVITATION FOR BIDS (IFB)
National Competitive Bidding (NCB) 
BIDDING DOCUMENT- PRICE PROPOSAL
Construction of new rathnapura showroom 
STC/PRO/SS/Rathnapura/2026/03
S/L STATE TRADING (GENERAL) CORPORATION LTD
NO:100, NAWAM MAWATHA

COLOMBO 02

INVITATION FOR BIDS
Sri Lanka State Trading (General) Corporation Limited.
Construction of new rathnapura showroom 
Closed Framework Agreement
Sri Lanka State Trading (General) Corporation Limited, a fully government-owned, self-financed corporation operating under the Ministry of Trade, Commerce, Food Security, and Cooperative Development, invites Price proposal from eligible and qualified bidders for Construction of new rathnapura showroom – STC/PRO/SS/Rathnapura/2026/03
If further information is required can be obtained from The Manager (Procurement), Sri Lanka State Trading (General) Corporation Ltd, No. 100, Nawam Mawatha, Colombo 02, Sri Lanka. on working days from 9.00 am to 4.00 pm. (Local Time) Telephone +94 11 2422341-4 Fax +94 11 2447970 Mobile – 0702-590305 
Please be informed that the Pre-Bid Meeting for the tender will be held on 14th October 2026 (Wednesday) at 11:00 a.m. All interested bidders are requested to attend the meeting.

Bid documents may be obtained from the Procurement Division of the Head Office of the Sri Lanka State Trading (General) Corporation Ltd from 8 October 2026 to 25 October 2026, on working days between 9:00 a.m. and 4:00 p.m., or download from the Corporation's website at https://www.stc.lk/rathnapura2026/03
All bids in given format to be handover on or before 28.10.2026 at 2.00PM (Colombo Time) Late bids shall not be accepted. Bidder must mark as “Proposed Expansion of Existing Formaldehyde Store” on left hand corner of the envelope
The Chairman, 
Sri Lanka State Trading (General) Corporation Ltd, 
100, Nawam Mawatha, Colombo 02,  Sri Lanka.
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VOLUME I I
· Section II. Bidding Data Sheet (BDS)

· Section III. Evaluation and Qualification Criteria

· Section IV. Bidding Forms

· Section V. Schedule of Requirements

· Section VII. Contract Data

· Invitation For Bid

VOLUME II

Section II. Bidding Data Sheet (BDS)
The following specific data for the goods to be procured shall complement, supplement, or amend the provisions in the Instructions to Bidders (ITB). Whenever there is a conflict, the provisions herein shall prevail over those in ITB.
	ITB Clause Reference
	A. General

	ITB 1.1
	The Purchaser is:- Sri Lanka State Trading (General) Corporation Limited, 100, Nawam Mawatha, Colombo 02, Sri Lanka.

	ITB 1.1
	The name and identification of the Procurement: - for Proposed Construction of new rathnapura showroom
The items should match with the specifications given in the bidding document 


	ITB 2.1
	The source of funding is:- State Trading (General) Corporation  funds in Sri Lanka

	ITB 4.1
	Eligibility for Bidding to " STC/PRO/SS/Rathnapura/2026/03"

	
	B. Contents of Bidding Documents

	ITB 7.1
	For clarifications Purchaser’s address: - 
  The Manager (Procurement),
State Trading (General) Corporation Limited 
No. 100, Nawam Mawatha,
Colombo 02, Sri Lanka
Telephone: +94 11 2422341-4     Fax +94 11 2447970 
Mobile – 0702 590305

	
	C. Preparation of Bids

	ITB 11.1(e)
	The bidder shall submit the relevant documents specified.

	ITB 13.1
	Alternative bids , Alternative bids shall not be considered.

	ITB 19.1
	The Bid shall be valid till 28th of January 2027 

	ITB 20.1
	Bid Security

1. Requirement:

Each bid must be accompanied by a Bid Security of Rs. 100,000.00 (Rupees One Hundred Thousand).
2. Form of Bid Security:

The Bid Security shall be in one of the following forms
Cash or Bank Guarantee issued by a licensed commercial bank in Sri Lanka 

3. Issuing Authority: 
For Bank Guarantee: Must be issued by a recognized commercial bank acceptable to the Employer

4. Validity:

The Bid Security must remain valid for a minimum of 91 days from the bid closing date, or until the contract is awarded and the Performance Security is provided.

5. Return of Bid Security:

Unsuccessful bidders: Bid Security will be returned within 30 days of contract award

Successful bidder: Bid Security will be returned upon receipt and acceptance of the Performance Security

6. Forfeiture:

The Bid Security will be forfeited if the bidder:

Withdraws the bid during the validity period

Fails to accept the contract when awarded

Fails to provide the required Performance Security



	
	D. Submission and Opening of Bids

	ITB
22.1
	Addressed to 
The Chairman , ,

Sri Lanka State Trading ( General) Corporation  Ltd, 
100, Nawam Mawatha,

Colombo 02, Sri Lanka.

	ITB 23.1
	Address for submission of Quotations is:
Chairman, State Trading (General) Corporation Limited, No. 100, Nawam Mawatha,

Colombo 02, Sri Lanka
Deadline for submission of quotations is: 1400 Hrs (02.00 P.M) on October 28, 2026
Envelope containing the quotation should be marked “Construction of new rathnapura showroom - STC/PRO/SS/Rathnapura/2026/03”

	
	E. Evaluation and Comparison of Bids       

	ITB 34.1
	Domestic preference shall not be a bid evaluation factor.

	ITB 35.4
	The Purchaser’s evaluation of a bid will be based on technical ability and evaluated bid price. The bidder is expected to do system demonstration according to the minimum specifications in the bidding documents. If the bidder fails to demonstrate minimum specifications required by the bidding documents may be rejected by the purchaser as non-respective.
The following factors and methodology will be used for evaluation: 
Eligibility for Bidding to " STC/PRO/SS/Rathnapura/2026/03"

1.  Preliminary Evaluation 
          1.1 Submission of signed Form of Bid
2. Detailed Evaluation
i.
 Bidder shall be a legally registered company in Sri Lanka and has been in operation for the last five (05) years.

ii.
Chartered architects registered with CIDA (Construction Industry Development Authority) Category C-7 or above qualification would be added advantage.
iii.
Detailed list of similar projects/orders that the bidder has completed successfully during the period of last three (03) years ending on the deadline of bid submission.

iv.
Bidders and agents shall have experience as the authorized dealers/suppliers for brands/products offered in the bid for the last 3 years in supply, delivery installation, providing warranty and maintenance.

iv. Bidder shall have skilled and technically competent team to carry out necessary warranty, support, and maintenance and after sales services.

v.
Documentary evidence to establish conformity of the goods to the technical specifications/standards in the bidding documents along with the Technical Specification Form.
Specifications
         3.2. Work completion schedule   
         3.3 Prices of the items & Warranty periods.


Section III.  

Evaluation and Qualification Criteria 

This Section complements the Instructions to Bidders. It contains the criteria that the Purchaser use to evaluate a bid and determine whether a Bidder has the required qualifications. No other criteria shall be used.  

[The Purchaser shall select the criteria deemed appropriate for the procurement process, insert the appropriate wording using the samples below or other acceptable wording, and delete the text in italics] 

Contents 

1. Evaluation Criteria (ITB 35.3 {d}) 

2. Evaluation Criteria (ITB 35.4 

3. Multiple Contracts (ITB 35.5) 

4. Domestic Preference (ITB 34.1) 

5. Post qualification Requirements (ITB 37.2)

1. Evaluation Criteria (ITB 35.3 (d)) 

The Purchaser’s evaluation of a bid may take into account, in addition to the Bid Price quoted in accordance with ITB Clause 14, one or more of the following factors as specified in ITB Sub-Clause 35.3(d) and in BDS referring to ITB 35.3(d).

2. Evaluation Criteria (ITB 35.4)

A bid evaluation committee appointed by the Chairman, CWECE will evaluate the Bids in Accordance of ITB 35.45

Section IV.  Bidding Forms
Table of Forms
Bid Submission Form ............................................................................................................
Price Schedule: .......................................................................................................................
Bid Security (Guarantee) .....................................................................................................
                                                 Bid Submission Form
[The Bidder shall fill in this Form in accordance with the instructions indicated No alterations to its format shall be permitted and no substitutions shall be accepted.]
Date: 
No.: Proposed Construction of new rathnapura showroom
     STC/PRO/SS/Rathnapura/2026/03
To:
The Chairman,
Sri Lnka State Trading (General) Corporation Limited ,
 
No. 100, Nawam Mawatha,Colombo 02. Sri Lanka.
We, the undersigned, declare that:
a) We have examined and have no reservations to the Bidding Documents, 
b) We offer to supply in conformity with the Bidding Documents and in accordance with the completion time in the Schedule of Requirements 
c) The total price of our Bid, including any discounts offered is: [insert the total bid price in Figures………………………..Words…………………………………………………………………
d) Our bid shall be valid for the period of time specified in ITB Sub-Clause 19.1, from the date fixed for the bid submission deadline in accordance with ITB Sub Clause 23.1, and it shall remain binding upon us and may be accepted at any time before the expiration of that period;
e) If our bid is accepted, we commit to obtain a performance security in accordance with ITB Clause 43 and CC Clause 17 for the due performance of the Contract;
f) We have no conflict of interest in accordance with ITB Sub-Clause 4.3;
g) Our firm, its affiliates or subsidiaries including any subcontractors or suppliers  for any part of the contract has not been declared blacklisted by the National Procurement Agency/ Department of Public Finance of Sri Lanka;
h) We understand that this bid, together with your written acceptance thereof included in your notification of award, shall constitute a binding contract between us, until a formal contract is prepared and executed.
i) We understand that you are not bound to accept the lowest evaluated bid or any other bid that you may receive.
Signed:…………………………………………………

    Name : ……………………………………………… [insert signature of person whose name and capacity are shown]
In the capacity of …………………………………………………………………………. [insert legal capacity of person signing the Bid Submission Form]
Name of the Bidder :………………………………………………………………………. [insert complete name of person signing the Bid Submission Form]
Duly authorized to sign the bid for and on behalf of:
[insert complete name of Bidder]
Dated on
day of
,
[insert date of signing]
Contact Details
:
Mobile Number
:
QUALIFICATION INFORMATION
(To be completed by the bidder and submitted with the Bid)
	
	Eligibility Requirement
	Bidder’s Qualification

	ICTAD Registration
	
	

	Registration Number
	
	

	
Grade
	C7 above
	

	Expiry Date
	Valid ICTAD registration
	

	Black listed contractors
	

	Have you been declared as a defaulted contractor by NPA or any other Agency?
	
	Yes / No

	If yes provide details.
	
	

	VAT Registration Number
	
	

	Construction Program
	(attach as annex)

	Legal Status
	(Public Company/Private Company/Partnership/Sole Proprietor)

	Qualification and experience of key staff
	Eligibility Requirement
	Bidder’s Qualification

	
	Category, Experience and Qualifications
	Required Nos
	

	
	1. Site Supervisor With one Year Experience
	01
	

	
	
	
	

	
	
	
	

	List other information required
	


Signature of the Bidder: ……………………………………….
PRICE SCHEDULE
PROPOSED CONSTRUCTION OF NEW RATHNAPURA SHOWROOM AT  

SRI LANKA STATE TRADING (GENARAL) CORPORATION COLOMBO 02

	No.
	Description
	 
	Amount (LKR)

	01
	Removing and transport of existing Containers
	
	

	02
	Excavation
	
	

	03
	Concrete Work & Reinforcements
	
	

	04
	Steel Iron Structure
	
	

	05
	Fabricate and Installation of Steel Staircase.
	
	

	06
	Painting
	
	

	07
	Roof Works
	
	

	08
	Rain water gutters and down pipes
	
	

	09
	Electrical Installations
	
	

	10
	Floor and Wall Finishes
	
	

	11
	Ceiling Works
	
	

	12
	Door & Windows
	
	

	 A
	Sub Total  
	
	

	 B
	Discount   ..... % [percentage of subtotal A or specified items (pl. Specify the items) , if given]

.........................................................................................
	

	TOTAL BID PRICE, CARRIED TO LETTER OF BID 
	

	Total Bid Price (Amount in words) :-
	 
	

	VAT- 18% of Bid Price
	

	GRAND TOTAL INCLUDING VAT 
	


…………………………….            ………………….      ………………………………..

Signature of the Bidder

Date                          Company Seal
Please place the signature and the company embossed seal
PROPOSED EXPANSION OF EXISTING FORMALDEHYDE STORE AT

SRI LANKA STATE TRADING (GENARAL) CORPORATION  
COLOMBO 02
	Item No
	Description
	Unit
	Qty
	Rate
	Amount

	 
	Removing and transport of existing Containers
	 
	 
	 
	 

	1
	Safe dismantling, removal and transportation of the existing 40 ft long container unit currently installed at the Sri Lanka Foundation, Colombo 07, to the new site in Ratnapura. Prior to dismantling and removal of the container unit, all existing glass panels shall be carefully dismantled, removed and safely transported. Tree branches obstructing the removal and transportation of the container shall be properly cut and removed as necessary. The container unit shall then be safely dismantled, removed from the existing location and transported to the designated new site in Ratnapura, including all necessary labour, equipment, lifting, handling and transportation.
	Item 
	Allow
	 Sum 
	 

	2
	Safe dismantling, removal and transportation of the existing 40 ft long container unit currently installed at the Borella, to the new site in Ratnapura. Prior to dismantling and removal of the container unit, all existing glass panels shall be carefully dismantled, removed and safely transported. The container unit shall then be safely dismantled, removed from the existing location and transported to the designated new site in Ratnapura, including all necessary labour, equipment, lifting, handling and transportation.
	Item 
	Allow
	 Sum 
	 

	3
	Safe dismantling, removal and transportation of the existing 40 ft long container unit currently installed at the Padukka, to the new site in Ratnapura. Prior to dismantling and removal of the container unit, all existing glass panels shall be carefully dismantled, removed and safely transported. The container unit shall then be safely dismantled, removed from the existing location and transported to the designated new site in Ratnapura, including all necessary labour, equipment, lifting, handling and transportation.


	Item 
	Allow
	Sum 
	 

	Item No
	Description
	Unit
	Qty
	Rate
	Amount

	4
	Carefully dismantle, remove and transport the existing 40 ft long container unit currently installed in the Homagama area to the designated new site in Ratnapura. Prior to dismantling, all existing glass panels shall be carefully removed, protected and safely transported to the new site. Where necessary, provide and install temporary internal steel bracing/support frames to maintain the structural integrity and stability of the container during dismantling and lifting operations. The entire operation shall be carried out without causing damage or deformation to the container frame/structure, including all necessary labour, temporary steelwork, lifting equipment, loading, transportation, unloading, handling and safety measures,
	Item 
	Allow
	 Sum 
	 

	 
	Excavation
	 
	 
	 
	 

	5
	Excavation of 3'-0"x3'-0"x2'-0" size columns pits as per drawing in any material total depth not exceeding 1.0m
	Cuft
	288.0
	 
	 

	 
	Concrete Work & Reinforcements
	 
	 
	 
	 

	6
	Insitue Concrete 3" Thk.1:3:6 (1") mass concrete for 16 Nos. of new column bases.
	Cuft
	36.0
	 
	 

	7
	Insitue Concrete 1:2:4(3/4") for column base and column shaft as per drawing. 
	Cuft
	125.0
	 
	 

	8
	Supplying, bending and placing 12mm tor steel for column base.
	kg
	120.0
	 
	 

	9
	Supplying, bending and placing 16mm tor steel for column shafts.
	kg
	161.0
	 
	 

	10
	Supplying, bending and placing 6mm mild steel for column shafts.
	kg
	15.0
	 
	 

	11
	Hiring 1'-0"x 1'-0" size steel box for concrete the column shafts.
	Item 
	Allow
	 Sum 
	 

	12
	Providing and constructing reinforced concrete tie beams of size 1'-0" × 9", using 1:2:4 (3/4") cement concrete mix, reinforced with 16 mm diameter main bars and 6 mm diameter stirrups at 8" c/c, connecting columns, including formwork, placing, compacting and curing, complete as shown in the drawings.


	Lft
	185.0
	 
	 

	 
	Steel Iron Structure
	 
	 
	 
	 

	13
	Provide and install 25 mm thick steel base plates on 1'-0" × 1'-0" concrete columns, securely fixed with anchor bolts, including welding of 200 × 200 × 8 × 12 mm steel H-sections vertically to the base plates and providing 200 × 200 × 8 × 12 mm steel H-sections horizontally to form the complete steel structural frame, all as shown on the drawings, including cutting, welding, fixing, alignment, painting and all necessary accessories and workmanship.
	Item 
	Allow
	 Sum 
	 

	14
	Construction of concrete entrance steps for building access as shown in the drawings, having lengths of 4'-6" and 6'-10" comprising of 2 steps, using 1:3:6 (1") cement concrete mix. Rate shall include for all necessary excavation, formwork (shuttering), compaction, and finishing all exposed surfaces with a smooth plaster using 1:3 cement-sand mortar as per instructions and drawings.(Rise: 6"  , Thread : 10")
	Item 
	Allow
	 Sum 
	 

	 
	Fabricate and Installation of Steel Staircase.
	 
	 
	 
	 

	15
	Supplying, fabricating, assembling, and hoisting in position of a structural steel staircase consisting of 16 steps (7" rise & 10" tread) as per the detailed drawing. Structure includes C 100x50x5x7.5mm steel channel stringers, H 125x125x6.5x9mm column supports, L 60x60x5mm angle irons, and FB 60x6mm flat bars for step fabrication. Connection to be done using PL 110x80x6mm, PL 115x80x6mm, PL 70x80x10mm, and PL 95x80x10mm MS plates with M14 bolts and nuts or structural welding. Rate shall include for cleaning, applying two coats of anti-corrosive primer, and two coats of approved enamel paint for all exposed steel surfaces.
	Item 
	Allow
	 Sum 
	 

	16
	Supplying and fixing of 1½" Diameter Stainless Steel (S/S) Top Rail and mid-rails as balustrades/handrails for the staircase including necessary loops, end caps, and welding joints polished to a neat finish as per drawing details.

	Lft
	25.0
	 
	 

	17
	Supplying and laying of Stone Plastic Composite (SPC) floor finish on all staircase treads and landings including necessary nosing profiles, surface preparation, and approved adhesive work complete.

	Sqft
	45.0
	 
	 

	 
	Painting
	 
	 
	 
	 

	18
	Preparing external corrugated Corten steel surfaces of the container including high-pressure water washing to remove dirt, grease, and salt deposits; removing existing commercial stickers/decals; wire brushing and mechanical grinding to remove loose paint and rust patches down to bare metal; applying an approved rust converter on rusted areas; applying one coat of heavy-duty Marine-grade Epoxy Primer; and finishing with two coats of premium Marine-grade Polyurethane (PU) matt paint using an airless spray system or approved method. complete as per architectural specifications and instructions.
	Sqft
	1110.0
	 
	 

	 
	Roof Works
	 
	 
	 
	 

	 
	Steel Structures
	 
	 
	 
	 

	19
	Supply, fabrication, and installation of a Zinc-Aluminium (Amano) roofing sheets to cover the top of containers as per the drawings. Framework shall be constructed using 2.0mm thick heavy duty GI box bars, aligned vertically and horizontally, and securely joined by welding. Roofing sheets shall be 0.47mm thick Zinc-Aluminium (Amano), fixed to the steel framework using approved roofing screws. All exposed GI box bars shall be prepared and applied with two coats of approved quality and color enamel paint over a suitable primer coat, all complete as directed by the Engineer.
	Sqft
	1200.0
	 
	 

	 
	Rain water gutters and down pipes
	 
	 
	 
	 

	20
	Gutters, eaves 150mm G.I semicircular 22 B.W.G making and fixing with hooks or brackets and screws, and joints to be soldered complete.
	Lft
	80.0
	 
	 

	21
	Making and fixing Downpipes 150 mm (6") dia. Using G.I, 22 B.W.G with holdfasts or plugs fixed to steel columns and connect to main drain line. Excavation 8"x8" size trench for laying and connect to main drail line.

	Lft
	50.0
	 
	 

	 
	Electrical Installations
	 
	 
	 
	 

	22
	Supply and installation of pendent lamp with 2x1mm2 PVC/PVC/CU + 2.5mm2 PVC/CU earth cable terminated in a 3 terminal ceiling rose and sunk switch, wired in concealed conduit and connect to main electrical wiring system.
	Nos
	25.0
	 
	 

	23
	Supply and installation of water resist wall lamps with 2x1mm2 PVC/PVC/CU + 2.5mm2 PVC/CU earth cable terminated in a 3 terminal ceiling rose and sunk switch, wired in concealed conduit and connect to main electrical wiring system.
	Nos
	5.0
	 
	 

	24
	13 AMP switch socket outlet wiring to be carried out with 2C,2.5mm2 PVC/PVC/CU + 2.5mm2 PVC/CU earth cable wired in concealed conduit in wall and above ceiling to be supplied and installed to working order
	Nos
	11.0
	 
	 

	25
	15 AMP switch socket outlet c/w 20A DP wiring to be carried out with 2C,2.5mm2 PVC/PVC/CU + 2.5mm2 PVC/CU earth cable wired in concealed conduit in wall and above ceiling to be supplied and installed to working order
	Nos
	8.0
	 
	 

	26
	6 Way TP & N Distribution Board complete with 40A 4P MCB (Main Switch) and 40A 4P RCD (30mA)
	Nos
	1.0
	 
	 

	27
	Supply, laying, and installation of 4C/16mm² Cu/PVC/PVC unarmoured main power cable from the main electricity meter panel to the distribution board (DB). The cable shall be drawn through heavy-duty PVC conduits, trunking, or surface clipped neatly along  steel structures using approved clips, including all necessary terminal lugs, glands, drilling through walls, sealing, testing, and commissioning, all complete as per the drawings and directed by the Engineer.
	Lft
	20.0
	 
	 

	28
	Supply, laying, connection, testing, and commissioning of 4-Core 10mm² CU/XLPE/PVC/SWA/PVC 600/1000V Armoured Cable as the main power line from the CEB main meter box to the indoor Main Distribution Board (DB).
	Lft
	30.0
	 
	 

	 
	Floor and Wall Finishes
	 
	 
	 
	 

	 
	Floor Finishes
	 
	 
	 
	 

	29
	Supply, delivery, and installation of premium heavy-duty Stone Plastic Composite (SPC) Click-Lock Flooring Panels of overall thickness 5.0mm (including a minimum 0.5mm heavy-use wear layer and factory-attached 1.0mm/1.5mm IXPE or EVA acoustic underlayment foam cushioning) for ground floor and upper floor area.
	Sqft
	1450.0
	 
	 

	 
	Wall Finishes
	 
	 
	 
	 

	30
	Preparing 1"x 1" GI box bar ( 4'-0" c/c vertically)  & 3/4" x3/4" GI box bar (2'-0" c/c Horizontal) frame for all internal faces of the container box (ground floor and upper floor) fixing with welding and supply and installation of 9mm Thk. WPC (Wood Plastic Composite) wall panels for box bar frame including cutting and finishing around corners, ensuring proper alignment and level finish.(WPC panel Color: Burma Teak with Black Line)
	Sqft
	2830.0
	 
	 

	 
	Ceiling Works
	 
	 
	 
	 

	31
	Supplying and fixing  gypsum board suspended ceiling, using 600mmx600mmx9mm. thick ceiling boards in white colour interlock type hot dip GI grid system , forming a panel side of 610mmx610mm, and 
suspended  on 4mm  GI hanging rods with spring clip to soffit of container box (Ground floor & Upper floor)
	Sqft
	1440.00
	 
	 

	 
	Door & Windows
	 
	 
	 
	 

	32
	Supply and fixing TD1 4'-0'' x 8'-0'' size (2 nr) 12mm clear float tempered glass double door,consisting with floor hinges (VVP or Kinlong, one year  warranty), Door handles (pair), door locks (one year warranty) and necessary  accessories and riverts , screws… etc.
	Sqft
	64.00
	 
	 

	33
	Supplying, fabricating & fixing Aluminium natural anodized paneled door AD2 size is 900x2100mm (1 nr). Door frame consisting top and side bars (76x32mm) with 18x11mm door stopper bar. Door sash consisting top bar (80x42mm), side bars (66x45mm hinges side, 70x45mm lock side), middle bar (100x42mm) and bottom bar (120x42mm). 16x15mm clip bar should be used for required bars. 4mm thick Al/PVC double side composite board for bottom panel and 5mm thick clear glass for top panel should be fixed include with 3 Nrs of 100x75mm Al hinges, Al natural anodized door handle (102x40mm) pair, Door lock ect. 
	Sqft
	42.00
	 
	 

	34
	Supplying, Fabricating & Fixing 11'-0'' x 7'-0'' size Aluminium Window - AW1 (1 nos.) with 1.5mm thick, 80mm depth Aluminium Framed(max. width 37.6mm) three panel fixed glass Window fixing to steel frame including necessary beadings.
	Sqft
	77.00
	 
	 

	35
	Supplying, Fabricating & Fixing 6'-0'' x 7'-0'' size Aluminium Window - AW2 (2 nos.) with 1.5mm thick, 80mm depth Aluminium Framed(max. width 37.6mm) Two panel fixed glass Window fixing to steel frame including necessary beadings.
	Sqft
	84.00
	 
	 

	36
	Supplying, Fabricating & Fixing 5'-0'' x 7'-0'' size Aluminium Window - AW3 (1 nos.) with 1.5mm thick, 80mm depth Aluminium Framed(max. width 37.6mm) two panel fixed glass Window fixing to steel frame including necessary beadings.
	Sqft
	35.00
	 
	 

	37
	Supplying, Fabricating & Fixing 8'-0'' x 7'-0'' size Aluminium Window - AW4 (1 nos.) with 1.5mm thick, 80mm depth Aluminium Framed(max. width 37.6mm) three panel fixed glass Window fixing to steel frame including necessary beadings.
	Sqft
	56.00
	 
	 

	 
	TOTAL 
	 


Section V. Schedule of Requirements
1. Technical Specification

2. Drawings
1. Technical Specifications
1. General Requirements

All materials used for the fabrication, finishing, and installation of fittings shall be quality and approved by STC.

2. Sample and approval
No material shall be procured, fabricated or installed without prior written approval of the STC.

3. Material Components
3.1 Frame and Structural Supports

· Frame shall be fabricated using Galvanized iron (GI) box bar section of specified size and thickness.

· Section shall be clean, straight, rust-free and properly welded.

· Lights Fittings, gas detectors & Other Fittings: All LED Ceiling lights should have 2 years warranty
4. Testing and hand over:
Spill collection tank should be testing at least two weeks before handing over the project. 

Drawings

3) Mode of payments:  
Maximum 30% Advance (Advanced Payment Bond required), 30% (After completion of  50%), 35%  Payment    after Completion, 5% Retention release after 6 months from the completion date.

(a) Our firm, its affiliates or subsidiaries—including any subcontractors or suppliers for any part of the contract—has not been declared blacklisted by the National Procurement Agency;

(b)
We understand that this bid, together with your written acceptance thereof included in your notification of award, shall constitute a binding contract between us, until a formal contract is prepared and executed

(b) We understand that you are not bound to accept the lowest evaluated price or any other bid that you may receive.

The following points system will be used for evaluating of the technical team and technical proposal:

Signed: ………………………………… 

In the capacity of ………………………………………… 

Name: ………………………………
 

Duly authorized to sign the Bid Form for and on behalf of: (Company name) 

…………………………………………………………………………………………..
Dated on ____________ day of __________________, _______ [insert date of signing] Place Official Stamp
Section VII.  Contract Data
The following Contract Data shall supplement and / or amend the Conditions of Contract (CC). Whenever there is a conflict, the provisions herein shall prevail over those in the CC.
	CC 1.1(i)
	The Chairman,
Sri Lanka State Trading (General) Corporation Ltd,

100, Nawam Mawatha,

Colombo 02, Sri Lanka


	CC 1.1 (m)
	Final Destination of Goods
Sri Lanka State Trading (General) Corporation Limited
 No 100, Nawam Mawatha, Colombo 02 
Sri Lanka
Via Colombo Port

	CC 8.1
	For notices, the Purchaser’s address shall be:
The Manager( Procurement)
Sri Lanka State Trading (General) Corporation Limited
No 100, Nawam Mawatha, Colombo 02,Sri Lanka
   Sri Lanka Telephone +94 11 2302042  Fax +94 11 2447970 email: trade@stc.lk. 

	CC 12.1
	The Purchaser’s evaluation of a bid will be based on technical ability and evaluated bid price. The bidder is expected to do system demonstration according to the minimum specifications in the bidding documents. If the bidder fails to demonstrate minimum specifications required by the bidding documents may be rejected by the purchaser as non-respective.
(a)
Financial Capability

The Bidder shall furnish documentary evidence that it meets the following financial requirements:

Minimum average annual turnover in last three (3) years shall be 1.5 times of the bid price.

Audited statements of accounts of the company for the past three (03) years shall be submitted with the bid
(b)
Commercial and Technical Capability

The Bidder shall furnish documentary evidence to demonstrate that it meets the following requirements;

i.   Bidder shall be a legally registered company in Sri Lanka and has been in operation for the last five (05) years.
ii. Chartered architects registered with CIDA (Construction Industry Development Authority) Category C-7 or above qualification would be added advantage.
iii. Detailed list of similar projects/orders that the bidder has completed successfully during the period of last three (03) years ending on the deadline of bid submission.
iv. Bidders and agents shall have experience as the authorized dealers/suppliers for brands/products offered in the bid for the last 3 years in supply, delivery installation, providing warranty and maintenance.

iv. Bidder shall have skilled and technically competent team to carry out necessary warranty, support, maintenance and after sales services.

v. Documentary evidence to establish conformity of the goods to the technical specifications/standards in the bidding documents along with the Technical Specification Form.

	CC 15.1
	Advance Payment  

Thirty (30) percent of the Contract Price shall be paid within Fourteen (14) days of signing of the Contract, and upon submission of claim and a bank guarantee for equivalent amount valid until the Goods are delivered and in the form provided in the bidding documents. Format of the Advance Payment Bank Guarantee is given in Section VIII- Contract Forms.

Final Payment 

Payment shall be made in Sri Lanka Rupees within thirty (30) days of presentation of claim supported by a certificate from the Purchaser declaring that the Goods have been delivered and that all other contracted Services have been performed.

	
	Bid Security

Particulars Details Amount Rs. 100,000.00 Form Cash or Bank Guarantee Issued By Licensed commercial bank (acceptable to Employer) Validity Minimum 91 days from bid closing date Return 30 days after contract award (unsuccessful bidders)

	CC 17.1
	A Performance Security shall be an amount equal to 5% of the contract price. The performance security of the joint venture shall be in the names of the joint venture partners. Performance Security shall be submitted within 14 days of the date of the notification of award from the purchaser and it shall be valid up to 30 days after the date of completion of supplier’s contract performance obligations including maintenance, warranty and providing support obligations.
The performance security will be released only upon satisfactory completion of the 37 months from the date of final acceptance of product and solution.

	
	Completion Period
The Contractor shall complete all works and achieve Practical Completion within ninety (90) calendar days from the date of handing over the site to the Contractor.


	CC 26.1
	Late Completion

The liquidated damages shall be 0.05% of the contract value per day.
The maximum amount of liquidated damages shall be 10% of the contact price.


Section VIII. Contract Forms
Table of Forms
1. Contract Agreement Format ( Signed After Awarding the Contract)
2. Performance Security Format ( To be submitted After Awarding the Contract)
Contract Agreement
THIS CONTRACT AGREEMENT is made
The …………… [insert: number ] day of
[Insert: month ], [Insert: year ].
BETWEEN
1) …………………………………………………………………………..……………… [Insert complete name of Purchaser], a [insert description of type of legal entity, for example, an agency of the Ministry of ..……………………………………………… or corporation and having its principal place of business at [Insert address of Purchaser]……………………………………………………………………….…… (hereinafter called “the Purchaser”), and
2)   [insert  name of Supplier],
a
corporation
incorporated
under
the
laws
of
[
insert:
country
of
Supplier
]
……………………………………................................................................................and
having
its
principal
place
of
business
at
[
insert:
address
of
Supplier]
………………………………………………… (hereinafter called “the Supplier”).
WHEREAS the Purchaser invited bids for certain Goods and ancillary services, viz., [insert  brief description of Goods and Services] ………………………………….. and has accepted a Bid by the Supplier for the supply of those Goods and Services in the sum of [insert Contract Price in words and figures, expressed in the Contract currency (ies)]
……………………….……………………………............... (hereinafter called “the Contract Price”).
NOW THIS AGREEMENT WITNESSETH AS FOLLOWS:
1. In this Agreement words and expressions shall have the same meanings as are respectively assigned to them in the Conditions of Contract referred to.
2. The following documents shall constitute the Contract between the Purchaser and the Supplier, and each shall be read and construed as an integral part of the Contract:
a. This Contract Agreement
b. Contract Data
c. Conditions of Contract
d. Technical Requirements (including Schedule of Requirements and Technical Specifications)
e. The Supplier’s Bid and original Price Schedules
f. The Purchaser’s Notification of Award
g. Add have any other documents
3. This Contract shall prevail over all other Contract documents. In the event of any discrepancy or inconsistency within the Contract documents, then the documents shall prevail in the order listed above.
4. In consideration of the payments to be made by the Purchaser to the Supplier as hereinafter mentioned, the Supplier hereby covenants with the Purchaser to provide the Goods and Services and to remedy defects therein in conformity in all respects with the provisions of the Contract.
5. The Purchaser hereby covenants to pay the Supplier in consideration of the provision of the Goods and Services and the remedying of defects therein, the Contract Price or such other sum as may become payable under the provisions of the Contract at the times and in the manner prescribed by the Contract.
IN WITNESS whereof the parties hereto have caused this Agreement to be executed in accordance with the laws of Democratic Socialist Republic of Sri Lanka on the day, month and year indicated above.
For and on behalf of the Purchaser
Signed: (insert signature) .…………………………………………………………………….
in the capacity of (insert title or other appropriate designation) …………………………
in the presence of (insert identification of official witness) …………………………..……
For and on behalf of the Supplier
Signed: (insert signature of authorized representative (5) of the supplier ……………..…
in the capacity of (insert title or other appropriate designation) …..………………………
in the presence of (insert identification of official witness) …………………………………
Performance Security
[Note: the purchaser is required to fill the information marked as “*” and delete this note prior to selling of the bidding document]
[The issuing agency, as requested by the successful Bidder, shall fill in this form in accordance with the instructions indicated]
----------------------------------------------------------[Issuing Agency’s Name, and Address of Issuing Branch or Office] 
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* Beneficiary: ------------------------------------------------[Name and Address of Employer] --------
[image: image3.png]



Date: 

PERFORMANCE SECURITY No.: 

We   have   been   informed   that
-----------------------------------------------[name   of   Supplier]
(hereinafter called “the Supplier”) has entered into Contract No. ----------------------------------
[reference number of the contract] dated
with you, for the
---------------------- supply of [name of contract and brief description] (hereinafter called “the Contract”).
Furthermore, we understand that, according to the conditions of the Contract, a performance guarantee is required.
At the request of the Supplier, we ------------------------------------- [name of Agency] hereby irrevocably undertake to pay you any sum or sums not exceeding in total an amount of -----------
------------------[amount in figures] (
) [amount in words], such sum being
payable in the types and proportions of currencies in which the Contract Price is payable, upon receipt by us of your first demand in writing accompanied by a written statement stating that the Contractor is in breach of its obligation(s) under the contract, without your needing to prove or to show grounds for your demand or the sum specified therein.
This guarantee shall expire, no later than the ………………….. day of ……………….., 20…..
[Insert date, 28 days beyond the scheduled completion date including the warranty period] and any demand for payment under it must be received by us at this office on or before that date.

[Signature(s)]
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